A B C D E F G H I J L O R T U V W

## C

Card - Class in javax.smartcardio
  A Smart Card with which a connection has been established.
Card() - Constructor for class javax.smartcardio.Card
  Constructs a new Card object.
CardChannel - Class in javax.smartcardio
  A logical channel connection to a Smart Card.
CardChannel() - Constructor for class javax.smartcardio.CardChannel
  Constructs a new CardChannel object.
CardException - Exception in javax.smartcardio
  Exception for errors that occur during communication with the Smart Card stack or the card itself.
CardException(String) - Constructor for exception javax.smartcardio.CardException
  Constructs a new CardException with the specified detail message.
CardException(Throwable) - Constructor for exception javax.smartcardio.CardException
  Constructs a new CardException with the specified cause and a detail message of `(cause==null ? null : cause.toString())`.
CardException(String, Throwable) - Constructor for exception javax.smartcardio.CardException
  Constructs a new CardException with the specified detail message and cause.
CardNotPresentException - Exception in javax.smartcardio
  Exception thrown when an application tries to establish a connection with a terminal that has no card present.
CardNotPresentException(String) - Constructor for exception javax.smartcardio.CardNotPresentException
  Constructs a new CardNotPresentException with the specified detail message.
CardNotPresentException(Throwable) - Constructor for exception javax.smartcardio.CardNotPresentException
  Constructs a new CardNotPresentException with the specified cause and a detail message of `(cause==null ? null : cause.toString())`.
CardNotPresentException(String, Throwable) - Constructor for exception javax.smartcardio.CardNotPresentException
  Constructs a new CardNotPresentException with the specified detail message and cause.
CardPermission - Class in javax.smartcardio
  A permission for Smart Card operations.
CardPermission(String, String) - Constructor for class javax.smartcardio.CardPermission
  Constructs a new CardPermission with the specified actions.
CardTerminal - Class in javax.smartcardio
  A Smart Card terminal, sometimes referred to as a Smart Card Reader.
CardTerminal() - Constructor for class javax.smartcardio.CardTerminal
  Constructs a new CardTerminal object.
CardTerminals - Class in javax.smartcardio
  The set of terminals supported by a TerminalFactory.
CardTerminals() - Constructor for class javax.smartcardio.CardTerminals
  Constructs a new CardTerminals object.
CardTerminals.State - Enum in javax.smartcardio
  Enumeration of attributes of a CardTerminal.
close() - Method in class javax.smartcardio.CardChannel
  Closes this CardChannel.
com.abc.terminalfactory - package com.abc.terminalfactory
  AB Circle USB TerminalFactory
CommandAPDU - Class in javax.smartcardio
  A command APDU following the structure defined in ISO/IEC 7816-4.
CommandAPDU(byte[]) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from a byte array containing the complete APDU contents (header and body).
CommandAPDU(byte[], int, int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from a byte array containing the complete APDU contents (header and body).
CommandAPDU(ByteBuffer) - Constructor for class javax.smartcardio.CommandAPDU
  Creates a CommandAPDU from the ByteBuffer containing the complete APDU contents (header and body).
CommandAPDU(int, int, int, int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes.
CommandAPDU(int, int, int, int, int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes and the expected response data length.
CommandAPDU(int, int, int, int, byte[]) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes and command data.
CommandAPDU(int, int, int, int, byte[], int, int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes and command data.
CommandAPDU(int, int, int, int, byte[], int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes, command data, and expected response data length.
CommandAPDU(int, int, int, int, byte[], int, int, int) - Constructor for class javax.smartcardio.CommandAPDU
  Constructs a CommandAPDU from the four header bytes, command data, and expected response data length.
connect(String) - Method in class com.abc.terminalfactory.AbCircleCardTerminalUSB
connect(String) - Method in class javax.smartcardio.CardTerminal
  Establishes a connection to the card.

A B C D E F G H I J L O R T U V W