# Index

A B C D E F G H I J L O R S T V W
All Classes and Interfaces|All Packages|Serialized Form

## G

getACKProtocolEnabledForReaders() - Method in class com.abc.bluetoothTerminalfactory.AbCircleBluetoothTerminalManager
  Flag indicating if the ACK protocol is enabled or not for connected readers that support it.
getActions() - Method in class javax.smartcardio.CardPermission
  Returns the canonical string representation of the actions.
getATR() - Method in class javax.smartcardio.Card
  Returns the ATR of this card.
getBasicChannel() - Method in class javax.smartcardio.Card
  Returns the CardChannel for the basic logical channel.
getBatteryLevel() - Method in class com.abc.bluetoothTerminalfactory.AbCircleCardTerminalBluetooth
  Gets the battery level from the reader as percentage (0xFF if charging)
getBatteryLevel(int) - Method in class com.abc.bluetoothTerminalfactory.AbCircleCardTerminalBluetooth
  Gets the battery level from the reader as percentage (0xFF if charging) or the voltage value in mV
getBytes() - Method in class javax.smartcardio.ATR
  Returns a copy of the bytes in this ATR.
getBytes() - Method in class javax.smartcardio.CommandAPDU
  Returns a copy of the bytes in this APDU.
getBytes() - Method in class javax.smartcardio.ResponseAPDU
  Returns a copy of the bytes in this APDU.
getCard() - Method in class javax.smartcardio.CardChannel
  Returns the Card this channel is associated with.
getChannelNumber() - Method in class javax.smartcardio.CardChannel
  Returns the channel number of this CardChannel.
getCLA() - Method in class javax.smartcardio.CommandAPDU
  Returns the value of the class byte CLA.
getCopyright() - Static method in class com.abc.bluetoothTerminalfactory.BluetoothSmartCard
  Returns the copyright information.
getData() - Method in class javax.smartcardio.CommandAPDU
  Returns a copy of the data bytes in the command body.
getData() - Method in class javax.smartcardio.ResponseAPDU
  Returns a copy of the data bytes in the response body.
getDefault() - Static method in class javax.smartcardio.TerminalFactory
  Returns the default TerminalFactory instance.
getDefaultType() - Static method in class javax.smartcardio.TerminalFactory
  Get the default TerminalFactory type.
getFirmwareVersion() - Method in class com.abc.bluetoothTerminalfactory.AbCircleCardTerminalBluetooth
  Returns the firmware version of the terminal as ASCII string
getHistoricalBytes() - Method in class javax.smartcardio.ATR
  Returns a copy of the historical bytes in this ATR.
getINS() - Method in class javax.smartcardio.CommandAPDU
  Returns the value of the instruction byte INS.
getInstance(Context) - Static method in class com.abc.bluetoothTerminalfactory.BluetoothSmartCard
  The getInstance() function is a static method that returns a singleton instance of the BluetoothSmartCard class
getInstance(String, Object) - Static method in class javax.smartcardio.TerminalFactory
  Returns a TerminalFactory of the specified type that is initialized with the specified parameters.
getInstance(String, Object, String) - Static method in class javax.smartcardio.TerminalFactory
  Returns a TerminalFactory of the specified type that is initialized with the specified parameters.
getInstance(String, Object, Provider) - Static method in class javax.smartcardio.TerminalFactory
  Returns a TerminalFactory of the specified type that is initialized with the specified parameters.
getMac() - Method in class com.abc.bluetoothTerminalfactory.DiscoveredReader
getManager() - Method in class com.abc.bluetoothTerminalfactory.BluetoothSmartCard
  This function returns the AbCircleBluetoothTerminalManager object that is used to communicate with bluetooth terminals devices
getName() - Method in class com.abc.bluetoothTerminalfactory.AbCircleCardTerminalBluetooth
getName() - Method in class com.abc.bluetoothTerminalfactory.DiscoveredReader
getName() - Method in class javax.smartcardio.CardTerminal
  Returns the unique name of this terminal.
getNc() - Method in class javax.smartcardio.CommandAPDU
  Returns the number of data bytes in the command body (Nc) or 0 if this APDU has no body.
getNe() - Method in class javax.smartcardio.CommandAPDU
  Returns the maximum number of expected data bytes in a response APDU (Ne).
getNr() - Method in class javax.smartcardio.ResponseAPDU
  Returns the number of data bytes in the response body (Nr) or 0 if this APDU has no body.
getP1() - Method in class javax.smartcardio.CommandAPDU
  Returns the value of the parameter byte P1.
getP2() - Method in class javax.smartcardio.CommandAPDU
  Returns the value of the parameter byte P2.
getProtocol() - Method in class javax.smartcardio.Card
  Returns the protocol in use for this card.
getProvider() - Method in class javax.smartcardio.TerminalFactory
  Returns the provider of this TerminalFactory.
GetReaderDiscoveryList() - Method in class com.abc.bluetoothTerminalfactory.AbCircleBluetoothTerminalManager
  This function returns a list of discovered readers
getSerialNumber() - Method in class com.abc.bluetoothTerminalfactory.AbCircleCardTerminalBluetooth
  Returns the serial number of the terminal as ASCII string
getSW() - Method in class javax.smartcardio.ResponseAPDU
  Returns the value of the status bytes SW1 and SW2 as a single status word SW.
getSW1() - Method in class javax.smartcardio.ResponseAPDU
  Returns the value of the status byte SW1 as a value between 0 and 255.
getSW2() - Method in class javax.smartcardio.ResponseAPDU
  Returns the value of the status byte SW2 as a value between 0 and 255.
getTerminal(String) - Method in class javax.smartcardio.CardTerminals
  Returns the terminal with the specified name or null if no such terminal exists.
getType() - Method in class javax.smartcardio.TerminalFactory
  Returns the type of this TerminalFactory.
getVersion() - Static method in class com.abc.bluetoothTerminalfactory.BluetoothSmartCard
  This function returns the version of the library

A B C D E F G H I J L O R S T V W
All Classes and Interfaces|All Packages|Serialized Form